Thank you for your interest in NoviiRemote Classic software for Palm OS!

This is a full unlimited version of the NoviiRemote Classic software,
ver 2.62, build 2006.01.17a, IR v64 (released in January 2006), 
ready for installation to Windows, Mac or Linux computers.

NEW !
 * Now palm TX and Z22 supported.
 * Learning on Cingular Treo 650 with 1.51/1.17 firmware supported.

1. Installation
===============

WARNING. The program does not yet support the following Sony Clie OS 5 devices: TJ series,
UX series, TH55, UK-50.

I M P O R T A N T. Do not remove the previous version of NoviiRemote from your handheld. 
You may lose your customized codebase. Just install the new version above the previous
one.

I M P O R T A N T. You must install only ONE prc-file, not all four presented in the
archive (see below). If you've installed the incorrect prc-file, just install the one
you need. The new file will write over the incorrect file on your handheld.

I M P O R T A N T. If you have a trial or previous version of NoviiRemote already
installed on your handheld, be careful with installing pdb-files presented in the
archive. pdb-files can overwrite your customized codebases. If necessary you may
compare the names of the codebases in this archive with the names of  the codebases
stored in your handheld, and install only those codebases you actually need.

The contents are as follows:

 * !readme.txt - this read-me instruction file.

 * NR_UserGuide_Palm262_iv.pdf 
   This is a User Guide in PDF format. 
   Do not install it on your handheld! This User Guide is designed for using on your
   desktop computer only. Put the User Guide into a convenient place, where you can
   access it again.

 * NoviiRemoteHelp.pdb
   This file must be installed on your handheld, and contains help information for use
   inside the NoviiRemote application.

 * NoviiRemoteHighRes.prc
   This is a color version of NoviiRemote software, high resolution (320*320), 1441 KB.
   Works on devices with high resolution display only (320*320), like palm TX, LifeDrive,
   Tungsten T, T2, T3, T5, C, W, E, E2, Zire 71, Zire 72, Treo 650, Tapwave Zodiac,
   Garmin iQue 3200, Garmin iQue 3600, etc.
   Demands several times more memory due to the hi-res graphics. If you are concerned
   about memory requirements, please install NoviiRemote on an expansion card, or select
   NoviiRemote 160*160.
   It does not work with Sony Clie devices running OS 4.x.
   It also works with many Sony Clie devices running OS 5.x: NX series, NZ series, TG-50.
   The program does not support the following Sony Clie OS 5 devices: TJ series,
   UX series, TH55, UK-50.

 * NoviiRemoteStandRes.prc
   This is a color version of NoviiRemote software, standard resolution (160*160), 646 KB.
   This version is best for work on devices with 160*160 color resolution, e.g. on Palm Z22,
   m130, Palm m515, Zire 31, Treo 600, Handsrping Treo and Visor devices.
   It can be also run on Tungsten T, T2, T3, T5, C, W, E, Zire 71, Zire 72, Treo 600, and
   other color devices with 320*320 resolution, and will occupy a smaller amount of memory
   on such handhelds. 
   It works with Sony Clie devices running OS 4.x
   It also works with many Sony Clie devices running OS 5.x: NX series, NZ series, TG-50.
   The program does not support the following Sony Clie OS 5 devices: TJ series,
   UX series, TH55, UK-50.

 * NoviiRemoteHighResSony.prc
   This is a color version of NoviiRemote software, high resolution (320*320), 1411 KB.
   Works on Sony Clie OS 4.x/5.v devices only, like NR70V, T665C, NX73V, NZ90, TG-50, etc. 
   Demands several times more memory due to the hi-res graphics. If you are concerned
   about memory requirements, please install NoviiRemote on a Memory Stick card, or select
   NoviiRemote 160*160
   It works with Sony Clie devices running OS 4.x
   It also works with many Sony Clie devices running OS 5.x: NX series, NZ series, TG-50.
   The program does not support the following Sony Clie OS 5 devices: TJ series,
   UX series, TH55, UK-50.

 * NoviiRemoteGray.prc
   This is a grayscale version of the NoviiRemote software, 506 KB.
   This version is best for grayscale devices like Palm Zire, Zire 21, m500, m125, i705,
   m100, Sony Clie T400C, etc.
   It can also be used on color devices, and will occupy a smaller amount of memory on
   such handhelds.
   It works with Sony Clie devices running OS 4.x
   It also works with many Sony Clie devices running OS 5.x: NX series, NZ series, TG-50.
   The program does not support the following Sony Clie OS 5 devices: TJ series,
   UX series, TH55, UK-50.

Important. You must install only ONE prc-file, not all four listed above. If you've
installed the incorrect prc-file, just install the one needed from the above list.
The new file will write over the incorrect file on your handheld.

 * A lot of pdb files in the IRdatabases folder.
   These are IR databases with infrared codes (called codebases) used for controlling
   popular home entertainment devices (TV, VCR, DVD, Audio, etc.). Please install them
   to your handheld  memory.

I M P O R T A N T. Do not install codebases on the SD card nor internal hard drive.

TIPS FOR INSTALLING IR CODEBASES:

1) When installing NoviiRemote software for the first time, it's best to install all the
codebases. Later you can easy remove unused codebases from your handheld.

2) Copy the pdb files in the IRdatabases folder to the internal memory of your handheld by
selecting all the files, then dragging and dropping them onto the Install window in your
Palm Desktop on your computer.

3) If you're not going to install all the codebases, please pay attention to the codebase
names. 
Prefix TV  denotes codebases used for controlling TV Sets,
prefix CAB denotes codebases used for controlling satellite and cable receivers,
prefix DVD denotes codebases used for controlling DVD and CD devices,
prefix VCR denotes codebases used for controlling VCR devices,
prefix Tiv denotes codebases used for controlling PVR/DVR devices like TiVo,
prefix AUD denotes codebases used for controlling audio devices (receivers, amplifiers, etc.).

4) Important. If you have a trial or previous version of NoviiRemote already installed on
your handheld, you should not install pre-built codebases. They can overwrite your customized
codebases.

5) We've created a forum where people who have lost their original remote controls or who
have broken remotes can download codebases created by other customers. Please visit our
website at the following address:

http://www.novii.tv/up/forum

and go to the NoviiRemote Codebase category. 

Please let us know if you need assistance with this installation. If you have any trouble
whatsoever, we'll be glad to help.

Any comments and suggestions are welcome.

We hope you enjoy our software, and are pleased to have you as our customer.

2. Getting Activation Key
==================

This is a complete full-functioned version. However without a registration pdb file, the 
application will stop its work ten days after the very first launch on your handheld.

To resume work of NoviiRemote you need an activation key. If you've already
ordered the application, you have got the activation key too.

If for some reason you have not got the activation key, you should register
NoviiRemote Classic by sending the proof of purchase to  service@novii.com. In response
you'll receive the activation key.

3. Technical support
====================

Please visit our web site at http://www.novii.tv/palm/classic for information about NoviiRemote
Classic Softawre, User Guide, FAQ, tutorials and other useful information.  If you cannot find
answers to your questions on our web site, please write to us at service@novii.com.

4. Contacts
===========

NoviiMedia

E-mail: service@novii.com 

Web: www.novii.tv
        www.novii.com

5. To purchase please refer to the PalmGear.com site.
==============

January 2006
The Novii Team
