Thank you for your interest in NoviiRemote!

This is a full unlimited version of the NoviiRemote software,
ver 2.4 (build 03.12.31b, released in January 2004), 
ready for installation to Windows, Mac or Linux computers.


I M P O R T A N T !! You must install only ONE prc-file, not all four presented in the archive.
If you've installed the incorrect prc-file, just install the one needed from the above list.
The new file will write over the incorrect file on your PDA.


The contents are as follows:

 * NRUserGuide_palm24_iv2.pdf. This is a User Guide in PDF format. 
   Do not install it on your PDA! This User Guide is designed for using on your desktop computer.

 * NoviiRemoteHelp.pdb. This file must be installed on your PDA, and contains help information for use
  inside the NoviiRemote application.

 * NoviiRemoteStandRes.prc. This is a color version of the NoviiRemote software, standard resolution (160*160), 530 KB.
  This version is best for work on devices with 160*160 color resolution, e.g. on Palm m130, Palm m515, etc.
  It can be also run on Tungsten T, T2, T3, C, W, E, Zire 71 and most Treo devices.
  It also works with Sony Clie devices running OS 4.x
  It does not work with Sony Clie devices running OS 5.x

 * NoviiRemoteHighRes.prc. This is a color version of the NoviiRemote software, high resolution (320*320), 1330 KB.
  Works on devices with high resolution display only (320*320), like Tungsten T, T2, T3, C, W, E, and Zire 71.
  Demands several times more memory due to the hi-res graphics. If you are concerned
  about memory requirements, please install NoviiRemote on an expansion card, or select NoviiRemote 160*160.
  It does not work with Sony Clie devices running OS 4.x/5.x

 * NoviiRemoteHighResSony.prc. This is a color version of the NoviiRemote software, high resolution (320*320), 1290 KB.
  Works on Sony Clie OS 4.x devices only, like NR70V, T665C, etc. 
  This version requires several times more memory due to the hi-res graphics. If you are concerned
  about memory requirements, please install NoviiRemote on a Memory Stick card, or select NoviiRemote 160*160
  It does not work with Sony Clie devices running OS 5.x

 * NoviiRemoteGray.prc. This is a grayscale version of the NoviiRemote software, 390 KB.
  Best for grayscale devices like Palm Zire, m500, m125, i705, m100, Sony Clie T400C,  etc.
  It can also be used on color devices, and will occupy a smaller amount of memory on such PDAs.

Important. You must install only ONE prc-file, not all four listed above. 
If you've installed the incorrect prc-file, just install the one needed from the above list.
The new file will write over the incorrect file on your PDA.

 * A lot of pdb files. These are IR databases with infrared codes used for controlling popular
   home entertainment devices (TV, VCR, DVD, Audio, etc.)

Important. If you have a trial or previous version of NoviiRemote already installed on your handheld, 
you should not install pdb-files. pdb-files can overwrite your customized codebases.

 * !readme.txt - this read-me instruction file.

Please let us know if you need assistance with this installation. If you have any trouble whatsoever,
we'll be glad to help.

Any comments and suggestions are welcome.

We hope you enjoy our software, and are pleased to have you as our customer.

Please visit our web site at http://www.novii.tv for information about our products,
User Guides, tutorials and other useful information.  If you cannot find answers to your
questions on our web site, please write to us at service@novii.com.

NoviiMedia

E-mail: service@novii.com 

Web: www.novii.tv
     www.novii.com
